/*!
    \file  readme.txt
    \brief description of the USART printf
*/

/*
    Copyright (C) 2017 GigaDevice

    2014-12-26, V1.0.0, platform GD32F1x0(x=3,5)
    2016-01-15, V2.0.0, platform GD32F1x0(x=3,5,7,9)
    2016-04-30, V3.0.0, firmware update for GD32F1x0(x=3,5,7,9)
    2017-06-19, V3.1.0, firmware update for GD32F1x0(x=3,5,7,9)
*/

  This demo is based on the GD32150R-EVAL/GD32190R-EVAL board, it shows how to retarget the C 
library printf function to the USART.

  The USARTx is configured as follow:
  - BaudRate = 115200 baud  
  - Word Length = 8 Bits
  - One Stop Bit
  - No parity
  - Hardware flow control disabled (RTS and CTS signals)
  - Receive and transmit enabled
  

